ASTERION S5.L1.A350.0W
Type: wall lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Light body: white painted steel plate.
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 4,8 W
Color temperature: 3000 K
Module luminous flux: 574 lm
Luminaire luminous flux: 433 lm
A: 350 mm
B: 165 mm
C: 175 mm
Dali 2: Available
Weight: 1500 g