JUNO LED ZK.K1.J3.XY
Type: suspension lamp. Lampshade: acrylic glass. Metal parts: painted aluminium in diverse colours, (combination) RAL 9003 (.31), RAL 3022 (.32), RAL 7021 (.33), RAL 6034 (.34), RAL 1018 (.35), RAL 7023 (.37), RAL 5009 (.38). Pendant: self-supporting white X-01 or black X-02 to X-23 cable reinforced with a steel wire.
Voltage: 230V
IK code: IK06
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 36 W
Color temperature: 3000 K
Module luminous flux: 4448 lm
Luminaire luminous flux: 3517 lm
A: 360 mm
B: 360 mm
C: 2000 mm
Dali 2: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Track system: Available on inquiry
Sádrokarton: Available on inquiry
Weight: 4400 g