MAIA A PMMA ZKS.L4A.M500.Y PA
Type: suspension lamp; ceiling lamp. Lampshade: acrylic glass PMMA. Metal parts: white painted steel plate. Pendant: self-supporting white cable reinforced with a steel wire.
Voltage: 230V
IK code: IK06
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 31,3 W
Color temperature: 4000 K
Module luminous flux: 5022 lm
Luminaire luminous flux: 4768 lm
A: 150 mm
B: 500 mm
C: 2000 mm
Dali 2: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Track system: Available on inquiry
Sádrokarton: Available on inquiry
Weight: 3400 g