DAPHNE ZT ZT.L5.D550.XY
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Pendant: white painted steel RAL 9003 (.31), chrome (.80), brass (.84), RAL chrom (.77) or RAL Argento dorato (.70) rod suspension.
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 26,7 W
Color temperature: 3000 K
Module luminous flux: 4020 lm
Luminaire luminous flux: 2893 lm
A: 550 mm
B: 245 mm
C: 1000 mm
Dali 2: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Track system: Available on inquiry
Weight: 8600 g