RETRO ZT ZT.L1.R19.XY
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9016 (.41), RAL 9005 (.45), RAL Copper (.72), RAL Bronze (.73), RAL Brass (.74) or RAL Chrom (.77). Pendant: rod.
Voltage: 230V
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 11,6 W
Color temperature: 3000 K
Module luminous flux: 1624 lm
Luminaire luminous flux: 1150 lm
A: 190 mm
B: 250 mm
C: 1000 mm
Dali 2: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Track system: Available on inquiry
Weight: 3000 g