DAPHNE ZL ZL3.L1.D351.31Y
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9003 (.31), RAL chrom (.77). Pendant: wire suspension with white cable.
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 16 W
Color temperature: 3000 K
Module luminous flux: 2412 lm
Luminaire luminous flux: 1872 lm
A: 350 mm
B: 160 mm
C: 2000 mm
D: max. 1000 mm
Dali 2: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Weight: 3500 g