TENDO PMMA S26.K2.TEZ2.Y
Type: ceiling and wall lamp. Lampshade: acrylic glass PMMA. Light body: white painted steel plate.
Voltage: 230V
Ballast: Driver
IK code: IK10
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 18,1 W
Color temperature: 4000 K
Module luminous flux: 2491 lm
Luminaire luminous flux: 1790 lm
A: 300 mm
B: 260 mm
C: 70 mm
D: 20 mm
Dali 2: Available
Bluetooth control: Available on inquiry
Weight: 1200 g