TENDO PMMA S33.K1.TEZ3.Y
Type: ceiling and wall lamp. Lampshade: acrylic glass PMMA. Light body: white painted steel plate.
Voltage: 230V
Ballast: Driver
IK code: IK10
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 36 W
Color temperature: 3000 K
Module luminous flux: 4448 lm
Luminaire luminous flux: 3335 lm
A: 370 mm
B: 330 mm
C: 70 mm
D: 20 mm
Dali 2: Available
Motion sensor: Available on inquiry
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Weight: 1900 g