TENDO PMMA S44.K3.TEZ4.Y
Type: ceiling and wall lamp. Lampshade: acrylic glass PMMA. Light body: white painted steel plate.
Voltage: 230V
Ballast: Driver
IK code: IK10
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 29 W
Color temperature: 3000 K
Module luminous flux: 3945 lm
Luminaire luminous flux: 2916 lm
A: 460 mm
B: 440 mm
C: 80 mm
D: 20 mm
Dali 2: Available
Motion sensor: Available on inquiry
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Weight: 2600 g