POLARIS ZKS.P ZKS.P6.400.XM
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9003 (.31), RAL 9005 (.61), RAL chrom (.77), chrome (.80) or brass (.84). Pendant: white or black self-carrying conductor reinforced with a steel wire.
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 48,5 W
Color temperature: 4000 K
Module luminous flux: 7800 lm
Luminaire luminous flux: 7020 lm
A: 400 mm
C: 2000 mm
Dali 2: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Weight: 6000 g