SEMILUNA ZT.L1.S150.XY
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9003 (.60), RAL 9005 (.61), RAL Bronze (.73) or RAL Chrom (.77). Pendant: rod.
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 6,2 W
Color temperature: 3000 K
Module luminous flux: 804 lm
Luminaire luminous flux: 482 lm
A: 150 mm
C: 1000 mm
Dali 2: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Weight: 1700 g