GEO ZK2.L2.GC.61R
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9005 (.61). Pendant: black cable.
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 6,2 W
Color temperature: 4000 K
Module luminous flux: 869 lm
Luminaire luminous flux: 736 lm
A: 400 mm
B: 955 mm
C: 1150 mm
D: 150 mm
Dali 2: Available
Track system: Available
Weight: 900 g