POLARIS ZK PE ZK.P2.600.XY PE
Type: suspension lamp. Lampshade: polyethylene opal PE. Metal parts: painted steel plate RAL 9003 (.31), RAL 9005 (.61), RAL chrom (.77), chrome (.80), stainless steel (.83) or brass (.84). Pendant: white or black self-carrying conductor reinforced with a steel wire.
Voltage: 230V
Ballast: Driver
IK code: IK10
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 48,5 W
Color temperature: 4000 K
Module luminous flux: 7800 lm
Luminaire luminous flux: 7176 lm
A: 600 mm
C: 2000 mm
Dali 2: Available
Motion sensor: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Weight: 8700 g