OMNIA GLASS ZL1.K1.N25.XY
Type: suspension lamp. Lampshade: hand-blown crystal glass with LED source /direct, indirect/ placed in metal housing and protected by opal diffusers. Metal parts: painted steel plate  RAL Copper (.72), RAL Bronze (.73) , RAL Brass (.74), RAL Gold (.71). Pendant: wire suspension with black cable.
Voltage: 230V
IK code: IK06
Ballast: Driver
CRI:  >90
LED life:  L80F10>72000 hodin
Watt: 9,5 W
Color temperature: 3000 K
Module luminous flux: 1349 lm
Luminaire luminous flux: 960 lm
A: 250 mm
B: 210 mm
C: 1790 mm
Dali 2: Available
Bluetooth control: Available on inquiry
Track system: Available on inquiry
Weight: 2400 g