NUPAR GLASS ZT.K1.NU3.XY
Type: suspension lamp. Lampshade: hand-blown crystal glass with LED source /direct, indirect/ placed in metal housing and protected by opal diffusers. Pendant: rod. Colour: RAL7016 (62); RAL Gold (71); RAL Copper (72); RAL Bronze (73); RAL Brass (74).
Voltage: 230V
IK code: IK06
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 9,5 W
Color temperature: 3000 K
Module luminous flux: 1349 lm
Luminaire luminous flux: 967 lm
A: 350 mm
B: 200 mm
C: 1430 mm
Dali 2: Available
Bluetooth control: Available on inquiry
Track system: Available on inquiry
Weight: 3500 g