IZAR R MAX ZL4.IR.L2.1200M.91Y
Type: suspension lamp. Lampshade: acrylic glass. Metal parts: white painted steel plate. Pendant: steel wire suspension with a transparent cable.
Voltage: 230V
IK code: IK06
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 174 W
Color temperature: 4000 K
Module luminous flux: 24820 lm
Luminaire luminous flux: 21600 lm
A: 1200 mm
B: 180 mm
C: 2000 mm
Dali 2: Available
Motion sensor: Available on inquiry
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Weight: 36000 g