CHARON PMMA S33.L1.CA3.Y
Type: ceiling and wall lamp. Lampshade: acrylic glass PMMA. Light body: white painted steel plate.
Voltage: 230V
IK code: IK06
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 21,3 W
Color temperature: 3000 K
Module luminous flux: 3216 lm
Luminaire luminous flux: 2296 lm
A: 375 mm
B: 330 mm
C: 135 mm
Dali 2: Available
Motion sensor: Available on inquiry
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Weight: 1900 g