CHARON PMMA S56.L2.CA6.Y
Type: ceiling and wall lamp. Lampshade: acrylic glass PMMA. Light body: white painted steel plate.
Voltage: 230V
IK code: IK06
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 42,7 W
Color temperature: 4000 K
Module luminous flux: 6952 lm
Luminaire luminous flux: 4871 lm
A: 600 mm
B: 560 mm
C: 175 mm
Dali 2: Available
Motion sensor: Available on inquiry
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Weight: 4000 g