CHARON IP44 PS24.L1.T12.Y
Type: ceiling and wall lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Light body: white painted steel plate.
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 10,7 W
Color temperature: 3000 K
Module luminous flux: 1608 lm
Luminaire luminous flux: 1092 lm
A: 280 mm
B: 240 mm
C: 125 mm
Dali 2: Available
Motion sensor: Available on inquiry
Bluetooth control: Available on inquiry
Weight: 1800 g