CHARON S29.L1.T135.Y
Type: ceiling and wall lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Light body: white painted steel plate.
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 21,3 W
Color temperature: 3000 K
Module luminous flux: 3216 lm
Luminaire luminous flux: 2215 lm
A: 360 mm
B: 290 mm
C: 130 mm
Dali 2: Available
Motion sensor: Available on inquiry
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Weight: 2800 g