POLARIS ZK PE ZK.11.400.XY PE
Type: suspension lamp. Lampshade: polyethylene opal PE. Metal parts: painted steel plate RAL 9003 (.31), RAL 9005 (.61), RAL chrom (.77), chrome (.80), stainless steel (.83) or brass (.84). Pendant: white or black self-carrying conductor reinforced with a steel wire.
Voltage: 230V
IK code: IK10
Socket: E27
Lamps: 1x150W(max 19W LED)
A: 400 mm
C: 2000 mm
Track system: Available on inquiry
Sádrokarton: Available on inquiry
Weight: 3200 g