POLARIS ZK PE ZK.P1.400.XY PE
Type: suspension lamp. Lampshade: polyethylene opal PE. Metal parts: painted steel plate RAL 9003 (.31), RAL 9005 (.61), RAL chrom (.77), chrome (.80), stainless steel (.83) or brass (.84). Pendant: white or black self-carrying conductor reinforced with a steel wire.
Voltage: 230V
Ballast: Driver
IK code: IK10
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 25,5 W
Color temperature: 3000 K
Module luminous flux: 3784 lm
Luminaire luminous flux: 3482 lm
A: 400 mm
C: 2000 mm
Dali 2: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Sádrokarton: Available on inquiry
Weight: 4200 g