POLARIS ZL PE ZL1.P1.400.XY PE
Type: suspension lamp. Lampshade: polyethylene opal PE. Metal parts: painted steel plate RAL 9003 (.31), RAL chrom (.77) or chrome (.80). Pendant: steel wire suspension with a transparent cable.
Voltage: 230V
Ballast: Driver
IK code: IK10
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 25,5 W
Color temperature: 3000 K
Module luminous flux: 3784 lm
Luminaire luminous flux: 3482 lm
A: 400 mm
C: 2000 mm
Dali 2: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Track system: Available on inquiry
Sádrokarton: Available on inquiry
Weight: 4100 g