MAIA PMMA S1.L1W.Y PA
Type: wall lamp. Lampshade: acrylic glass PMMA opal. Light body: white painted steel plate.
Voltage: 230V
IK code: IK06
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 13,8 W
Color temperature: 3000 K
Module luminous flux: 1606 lm
Luminaire luminous flux: 1441 lm
A: 150 mm
B: 300 mm
C: 75 mm
Dali 2: Available
Motion sensor: Available on inquiry
Weight: 1200 g