MAIA A ZKS.L4A.M500.Y
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: white painted steel plate. Pendant: white cable.
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 31,3 W
Color temperature: 4000 K
Module luminous flux: 5022 lm
Luminaire luminous flux: 4139 lm
A: 150 mm
B: 500 mm
C: 2000 mm
Dali 2: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Track system: Available on inquiry
Sádrokarton: Available on inquiry
Weight: 4600 g