ELIOS ZK.11.E120.XY
Type: suspension lamp. Lampshade: acrylic glass for LED. Metal parts: painted aluminium – RAL 9016 (.41), RAL 3004 (.42), RAL 7023 (.43), RAL 5000 (.44) or RAL 9005 (.45). Pendant: transparent cable.
Voltage: 230V
IK code: IK06
Socket: E27
Lamps: 1x60W(max 9W LED)
A: 120 mm
B: 135 mm
C: 1500 mm
Track system: Available on inquiry
Weight: 550 g