POLARIS ZL ZL1.P3.500.XY
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9003 (.31), RAL chrom (.77) or chrome (.80). Pendant: steel wire suspension with a transparent cable.
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 48,5 W
Color temperature: 3000 K
Module luminous flux: 7216 lm
Luminaire luminous flux: 6494 lm
A: 500 mm
C: 2000 mm
Dali 2: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Track system: Available on inquiry
Weight: 7700 g