POLARIS ZTR ZTR.L1.200.XY
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9016 (.41), RAL 9005 (.45), RAL Copper (.72), RAL Bronze (.73), RAL Brass (.74) or RAL Chrom (.77). Pendant: rod.
Voltage: 230V
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 8,3 W
Color temperature: 3000 K
Module luminous flux: 1060 lm
Luminaire luminous flux: 967 lm
A: 200 mm
B: 225 mm
C: 1000 mm
Dali 2: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Track system: Available on inquiry
Weight: 2400 g