RETRO ZT ZT.11.R19.XY
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9016 (.41), RAL 9005 (.45), RAL Copper (.72), RAL Bronze (.73), RAL Brass (.74) or RAL Chrom (.77). Pendant: rod.
Voltage: 230V
Socket: E27
Lamps: 1x100W(max 13W LED)
A: 190 mm
B: 250 mm
C: 1000 mm
Track system: Available on inquiry
Weight: 3000 g