POLARIS S BS14.L2.200.XY
Type: ceiling and wall lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Light body: painted aluminium - RAL white 9016 (.41), RAL black 9005 (.45), RAL Copper (.72), RAL Bronze (.73) or RAL Brass (.74).
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 8,3 W
Color temperature: 4000 K
Module luminous flux: 1146 lm
Luminaire luminous flux: 1044 lm
A: 200 mm
B: 140 mm
C: 210 mm
Dali 2: Available
Weight: 1700 g