POLARIS S BS24.L2.350.XY
Type: ceiling and wall lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Light body: painted aluminium - RAL white 9016 (.41), RAL black 9005 (.45), RAL Copper (.72), RAL Bronze (.73) or RAL Brass (.74).
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 15,7 W
Color temperature: 4000 K
Module luminous flux: 2303 lm
Luminaire luminous flux: 2072 lm
A: 350 mm
B: 240 mm
C: 345 mm
Dali 2: Available
Motion sensor: Available on inquiry
Bluetooth control: Available on inquiry
Weight: 3600 g