IZAR METAL I2.L2.320.XY
Type: wall lamp. Lampshade: acrylic glass in combination with painted steel plate - RAL 9003, RAL 7021, RAL 6034, RAL 1018, RAL Copper, RAL Bronze, RAL 7023 or RAL 5009. Light body: white painted steel plate.
Voltage: 230V
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 9,1 W
Color temperature: 4000 K
Module luminous flux: 1278 lm
Luminaire luminous flux: 1111 lm
A: 320 mm
B: 80 mm
C: 40 mm
Dali 2: Available
Weight: 800 g