DAPHNE ZL ZL3.12.D351.31
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9003 (.31), RAL chrom (.77). Pendant: wire suspension with white cable.
Voltage: 230V
IK code: IK01
Socket: E27
Lamps: 2x60W(max 9W LED)
A: 350 mm
B: 160 mm
C: 2000 mm
D: max. 1000 mm
Weight: 3500 g