GEO ZK4.L1.G100.61Y
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9005 (.61). Pendant: black cable.
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 18,1 W
Color temperature: 3000 K
Module luminous flux: 2696 lm
Luminaire luminous flux: 2303 lm
A: 1700 mm
B: 950 mm
C: 150 mm
D: 150 mm
Dali 2: Available
Bluetooth control: Available on inquiry
Weight: 5500 g