ZED ZL3.L2.Z80.XY
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9003 (.60) or RAL 9005 (.61). Pendant: white or black cable.
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 27,2 W
Color temperature: 4000 K
Module luminous flux: 4368 lm
Luminaire luminous flux: 3680 lm
A: 900 mm
B: 550 mm
C: 1000 mm
Dali 2: Available
Bluetooth control: Available on inquiry
Weight: 8000 g