ZED ZL5.L1.Z100.XY
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9003 (.60) or RAL 9005 (.61). Pendant: white or black cable.
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 45,3 W
Color temperature: 3000 K
Module luminous flux: 6740 lm
Luminaire luminous flux: 5662 lm
A: 1050 mm
B: 570 mm
C: 1130 mm
Dali 2: Available
Bluetooth control: Available on inquiry
Weight: 11700 g