MAIA B ZK.L1B.M800.Y
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: white painted steel plate. Pendant: self-supporting white cable reinforced with a steel wire.
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 109,9 W
Color temperature: 3000 K
Module luminous flux: 14468 lm
Luminaire luminous flux: 10845 lm
A: 220 mm
B: 800 mm
C: 2000 mm
Dali 2: Available
Bluetooth control: Available on inquiry
Track system: Available on inquiry
Weight: 8300 g