ZED ZK2.11.ZC.XR
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9003 (.60) or RAL 9005 (.61). Pendant: white or black cable.
Voltage: 230V
IK code: IK01
Socket: G9
Lamps: 1x33W+1x48W(max 2x5W LED)
A: 400 mm
B: 955 mm
C: 1320 mm
Track system: Available
Weight: 1600 g