ZED ZK2.L2.ZD.XY
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9003 (.60) or RAL 9005 (.61). Pendant: white or black cable.
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 10,1 W
Color temperature: 4000 K
Module luminous flux: 1456 lm
Luminaire luminous flux: 1223 lm
A: 400 mm
B: 955 mm
C: 1320 mm
Dali 2: Available
Sádrokarton: Available
Weight: 1800 g