PRIMA BS14.K2.P14.XY
Type: ceiling and wall lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Light body: painted aluminium RAL 9016 (.41), RAL 9005 (.45), RAL Argento dorato (.70), RAL Bronze (.73) or RAL Brass (.74).
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 9,6 W
Color temperature: 4000 K
Module luminous flux: 1295 lm
Luminaire luminous flux: 868 lm
A: 140 mm
B: 100 mm
Dali 2: Available
Bluetooth control: Available on inquiry
Weight: 900 g