PRIMA BS44.K1.P44.XY
Type: ceiling and wall lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Light body: painted aluminium RAL 9016 (.41), RAL 9005 (.45), RAL Argento dorato (.70), RAL Bronze (.73) or RAL Brass (.74).
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 44,5 W
Color temperature: 3000 K
Module luminous flux: 5810 lm
Luminaire luminous flux: 3892 lm
A: 440 mm
B: 130 mm
Dali 2: Available
Motion sensor: Available on inquiry
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Weight: 4400 g