SEMILUNA SR.L2.S200.XY
Type: wall lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9003 (.60), RAL 9005 (.61), RAL Bronze (.73) or RAL Chrom (.77).
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 8,3 W
Color temperature: 4000 K
Module luminous flux: 1146 lm
Luminaire luminous flux: 688 lm
A: 340 mm
B: 200 mm
C: 250 mm
Dali 2: Available
Weight: 3200 g