CASTOR PS2.L4.XY
Type: wall lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Light body: painted steel plate RAL 9003 (.60), RAL 9005 (.61), RAL Argento dorato (.70),  RAL Bronze (.73), RAL Brass (.74).
IK code: IK01
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 9,1 W
Color temperature: 4000 K
Module luminous flux: 1278 lm
Luminaire luminous flux: 959 lm
A: 610 mm
B: 92 mm
C: 80 mm
D: 80 mm
Dali 2: Available
Bluetooth control: Available on inquiry
Weight: 3000 g