NOMIA BS44.K4.N44.XY
Type: ceiling and wall lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Light body: painted aluminium - RAL white 9003 (.31), RAL black 7021 (.33), RAL yellow 1018 (.35), RAL Argento dorato (.70) or RAL Gold (.71).
Voltage: 230V
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 29 W
Color temperature: 4000 K
Module luminous flux: 4133 lm
Luminaire luminous flux: 2769 lm
A: 440 mm
B: 80 mm
Dali 2: Available
Motion sensor: Available on inquiry
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Weight: 4400 g