MAIA S7.L1B.M320
Type: ceiling lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Light body: white painted steel plate.
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 14,5 W
Color temperature: 3000 K
Module luminous flux: 2007 lm
Luminaire luminous flux: 1503 lm
A: 150 mm
B: 320 mm
C: 360 mm
Dali 2: Available
Weight: 3200 g