CAPSULE ZL.L1.C15.XY
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted aluminum – RAL 7012 (.47), RAL 9003 (.60), RAL 9005 (.61), RAL 3012 (.75) or RAL 6011 (.76). Pendant: wire suspension with white or black cable.
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 6,2 W
Color temperature: 3000 K
Module luminous flux: 804 lm
Luminaire luminous flux: 482 lm
A: 170 mm
B: 270 mm
C: 2000 mm
Dali 2: Available
Track system: Available on inquiry
Sádrokarton: Available on inquiry
Weight: 2100 g