IZAR C ZL1.IC.K2.150.91Y
Type: suspension lamp. Lampshade: acrylic glass. Light body: white painted steel plate. Pendant: steel wire suspension with a transparent cable.
Voltage: 230V
IK code: IK06
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 9,6 W
Color temperature: 4000 K
Module luminous flux: 1295 lm
Luminaire luminous flux: 1070 lm
A: 150 mm
B: 150 mm
C: 2000 mm
D: 150 mm
Dali 2: Available
Motion sensor: Available
Emergency module: Available on inquiry
Bluetooth control: Available
Track system: Available on inquiry
Sádrokarton: Available on inquiry
Weight: 1300 g