IZAR C IC.K2.250.X
Type: ceiling and wall lamp. Lampshade: acrylic glass, sides white (.91) or black (.93). Light body: white painted steel plate.
Voltage: 230V
IK code: IK06
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 18,5 W
Color temperature: 4000 K
Module luminous flux: 2529 lm
Luminaire luminous flux: 2016 lm
A: 250 mm
Dali 2: Available
Motion sensor: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Track system: Available
Weight: 2200 g