FORUM ZL3.K2.O60.Y
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9006 structured. Pendant: steel wire suspension with a transparent cable.
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 50,8 W
Color temperature: 4000 K
Module luminous flux: 6975 lm
Luminaire luminous flux: 5369 lm
A: 600 mm
B: 100 mm
C: 2000 mm
Dali 2: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Weight: 9000 g