LEDA S37.L2.JS41.Y
Type: ceiling and wall lamp, type S37.xxx only as the ceiling lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Light body: white painted steel plate.
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 26,7 W
Color temperature: 4000 K
Module luminous flux: 4345 lm
Luminaire luminous flux: 2794 lm
A: 415 mm
B: 370 mm
C: 235 mm
Dali 2: Available
Motion sensor: Available on inquiry
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Weight: 4200 g